- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_dot_prod_q15.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_dot_prod_q15.c
    00009 *
    00010 * Description:  Q15 dot product.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * -------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00061 void arm_dot_prod_q15(
    00062   q15_t * pSrcA,
    00063   q15_t * pSrcB,
    00064   uint32_t blockSize,
    00065   q63_t * result)
    00066 {
    00067   q63_t sum = 0;                                 /* Temporary result storage */
    00068   uint32_t blkCnt;                               /* loop counter */
    00069
    00070 #ifndef ARM_MATH_CM0
    00071
    00072 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00073
    00074
    00075   /*loop Unrolling */
    00076   blkCnt = blockSize >> 2u;
    00077
    00078   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00079    ** a second loop below computes the remaining 1 to 3 samples. */
    00080   while(blkCnt > 0u)
    00081   {
    00082     /* C = A[0]* B[0] + A[1]* B[1] + A[2]* B[2] + .....+ A[blockSize-1]* B[blockSize-1] */
    00083     /* Calculate dot product and then store the result in a temporary buffer. */
    00084     sum = __SMLALD(*__SIMD32(pSrcA)++, *__SIMD32(pSrcB)++, sum);
    00085     sum = __SMLALD(*__SIMD32(pSrcA)++, *__SIMD32(pSrcB)++, sum);
    00086
    00087     /* Decrement the loop counter */
    00088     blkCnt--;
    00089   }
    00090
    00091   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00092    ** No loop unrolling is used. */
    00093   blkCnt = blockSize % 0x4u;
    00094
    00095   while(blkCnt > 0u)
    00096   {
    00097     /* C = A[0]* B[0] + A[1]* B[1] + A[2]* B[2] + .....+ A[blockSize-1]* B[blockSize-1] */
    00098     /* Calculate dot product and then store the results in a temporary buffer. */
    00099     sum = __SMLALD(*pSrcA++, *pSrcB++, sum);
    00100
    00101     /* Decrement the loop counter */
    00102     blkCnt--;
    00103   }
    00104
    00105
    00106 #else
    00107
    00108   /* Run the below code for Cortex-M0 */
    00109
    00110   /* Initialize blkCnt with number of samples */
    00111   blkCnt = blockSize;
    00112
    00113   while(blkCnt > 0u)
    00114   {
    00115     /* C = A[0]* B[0] + A[1]* B[1] + A[2]* B[2] + .....+ A[blockSize-1]* B[blockSize-1] */
    00116     /* Calculate dot product and then store the results in a temporary buffer. */
    00117     sum += (q63_t) ((q31_t) * pSrcA++ * *pSrcB++);
    00118
    00119     /* Decrement the loop counter */
    00120     blkCnt--;
    00121   }
    00122
    00123 #endif /* #ifndef ARM_MATH_CM0 */
    00124
    00125   /* Store the result in the destination buffer in 34.30 format */
    00126   *result = sum;
    00127
    00128 }
    00129

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines