Wizard Information Systems - IM-BAS Protocol Driver

==================================================================

   Copyright 2002 by Wizard Information Systems bv, The Netherlands. All rights reserved.

   FactoryLink is a registered trademark of United States Data Corporation, Richardson Texas USA.
   Wizard is a registered trademark of Wizard Information Systems bv, Rosmalen, The Netherlands

   This file contains the following sections:

           Installation

   For more information:

   Wizard Information Systems bv
   Pioenroosstraat 26
   5241 AB Rosmalen
   The Netherlands

   tel. + 31 73 523 1234
   fax  + 31 73 523 1222

==================================================================
***** Installation *****

Installation of the FactoryLink software.

First:

Install the files from the "Wizard IM_BAS driver" media to the appropriate directories. This is be done by running the setup utility placed on the installation media. 

Follow the next procedure:

{goto your installation media and directory} eg.: e:\im_bas
 type: setup, followed by enter

Second:

After you installed the software you need to activate the tables in the FactoryLink Configuration Explorer. The installation automatically appends the im-bas.ac entry into the {FLINK}/AC/titles file. The entry must match the im-bas.ac entry in the following table:

file: {FLINK}\ac\titles:

    ...
    spool.ac    
    itimer.ac   
    etimer.ac   
    decoder.ac  
    im_bas.ac 
    tiway_1.ac  
    ...

Third:

To make sure all the Configuration Tables (CT's) are generated after a change, the install utility automatically adds the im_bas entry at the end of the {FLINK}/ctgen/ctlist file. The place of this entry is not important. Check if this entry has the same format as in the next table:

file: {FLINK}\ctgen\ctlist:

    ...
    rpt: rptovr rpthdr
    im_bas: im_basm iso_basp iso_basd
    timer: itimer etimer
    ...

Fourth:

To enable the help fields in the IM-BAS configuration tables type the following command:

    {FLINK}\BIN\mkhelp

Fifth:

The FactoryLink Configuration Explorer uses a map file, {FLINK}/ac/ac2ct.map, to be aware of the different configuration tables which can be located behind one entry in the main menu. Upon startup, the Configuration Explorer reads the map file instead of all the table configuration files, mainly because reading all these files at once takes too much time. An account manager is present to update this conversion file, and can be started from the command line.

     {FLINK}\BIN\acctmgr  -c -d 

Sixth:

The im_bas task must be entered in the FactoryLink Configuration Manager (FLCM) System Configuration table. An entry of an existing task that will not be used at run-time can be overwritten or a new entry can be made with as a minimum the following data:

    Task Name   Description   ....                      Executable File

    IM_BAS      IM-BAS Protocol Driver                  bin/im_bas

The Task Name and Executable File name are fixed and should not be altered by the user.

***** Installation *****
==================================================================