{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PLC 02 - Productie"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PLC 02 - Productie","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,1,1,2]],"flags":["formulas_cached_only"]}
["PLC Selection"]
["Quantum","140 CPU 434 12",null,"64K Logic","32K State"]
["ICE"]
["  Runtime","Enabled"]
["  IEC Heap Size",620,"KB"]
["  Global Data",84,"KB"]
[]
["PLC Memory Partition"]
["Coils","000001","001536"]
["Discrete Inputs",100001,100512]
["Input Registers",300001,300512]
["Holding Registers",400001,408000]
[]
["Specials","On/Off","Waarde"]
["Battery Coil","Off","-"]
["Timer Register","Off","-"]
["Time Of Day","On",76]
["Allow Duplicate Coils","Off"]
["  First Coil Address","-"]
["Watchdog Timeout",null,30,"ms*10"]
["Online Editing Timeslice",null,20,"ms"]
[]
["Select Extensions"]
["Data Protection","Disabled"]
["Peer Cop","Disabled"]
["TCP/IP Ethernet",1]
["Symax Ethernet",0]
["MMS Ethernet",0]
["Profibus DP:",0]