                                                            SIMATIC S5 / COM 143
   SYSTEM IDENTIFIER    FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────

   CP TYPE    : CP 143        VERSION     : V 3.00

   PASSWORD   :               DATE        : 12-08-95

   BASE SSNR  :   0


   MEMORY TYPE: EPROM       MEMORY LENGTH : 60 KB


   ETHERNET ADDRESS: 080006010102 H
   
   
   

   DATA LINK BLOCK     FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────
   FROM LOCAL PLC:

   SSNR          :   0       ANR                 :   1
   JOB TYPE      : FETCH     ACTIVE/PASSIVE (A/P): P


   TO REMOTE PLC :

   ETHERNET ADDRESS : 000000000000 H    SSNR:         ANR:

      MULTICAST (Y/N): N   MULTICAST SET :     ETHERNET ADDRESS:              H

   DATAGRAM  (Y/N): N
   PRIORITY       : 2   READ/WRITE (Y/N): J


   SOURCE/DEST    :                LENGTH :
   STATUS WORD    :
   INTERPRETER    :                ADDRESS:      :      H


   LOCAL TSAP-ID  : LENGTH: 8     HEX: 57 49 5A 52 45 41 44 20  ASC: WIZREAD_
   REMOTE TSAP-ID : LENGTH: 8     HEX: 57 5A 50 53 41 43 50 55  ASC: WZPSACPU
   REMOTE NSAP-ID : LENGTH: 12   ASC :

   NUMBER OF JOBS PER TSAP      : 1
   
   
   DATA LINK BLOCK     FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────
   FROM LOCAL PLC:

   SSNR          :   0       ANR                 :   2
   JOB TYPE      : RECEIVE   ACTIVE/PASSIVE (A/P): P


   TO REMOTE PLC :

   ETHERNET ADDRESS : 000000000000 H    SSNR:         ANR:

   MULTICAST (Y/N): N   MULTICAST SET :     ETHERNET ADDRESS:              H

   DATAGRAM  (Y/N): N
   PRIORITY       : 2   READ/WRITE (Y/N): J


   SOURCE/DEST    :                LENGTH :
   STATUS WORD    :
   INTERPRETER    :                ADDRESS:      :      H


   LOCAL TSAP-ID  : LENGTH: 8     HEX: 57 49 5A 57 52 49 54 45  ASC: WIZWRITE
   REMOTE TSAP-ID : LENGTH: 8     HEX: 57 5A 50 53 41 43 50 55  ASC: WZPSACPU
   REMOTE NSAP-ID : LENGTH: 12   ASC :

   NUMBER OF JOBS PER TSAP      : 1

   
   DATA LINK BLOCK     FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────
   FROM LOCAL PLC:

   SSNR          :   1       ANR                 :   3
   JOB TYPE      : FETCH     ACTIVE/PASSIVE (A/P): P


   TO REMOTE PLC :

   ETHERNET ADDRESS : 000000000000 H    SSNR:         ANR:

   DATA LINK BLOCK     FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────
   FROM LOCAL PLC:

   SSNR          :   1       ANR                 :   3
   JOB TYPE      : FETCH     ACTIVE/PASSIVE (A/P): P


   TO REMOTE PLC :

   ETHERNET ADDRESS : 000000000000 H    SSNR:         ANR:


   DATA LINK BLOCK     FOR MODULE    :
────────────────────────────────────────────────────────────────────────────────
   FROM LOCAL PLC:

   SSNR          :   1       ANR                 :   4
   JOB TYPE      : RECEIVE   ACTIVE/PASSIVE (A/P): P


   TO REMOTE PLC :

   ETHERNET ADDRESS : 000000000000 H    SSNR:         ANR:

   MULTICAST (Y/N): N   MULTICAST SET :     ETHERNET ADDRESS:              H

   DATAGRAM  (Y/N): N
   PRIORITY       : 2   READ/WRITE (Y/N): J


   SOURCE/DEST    :                LENGTH :
   STATUS WORD    :
   INTERPRETER    :                ADDRESS:      :      H


   LOCAL TSAP-ID  : LENGTH: 8     HEX: 57 49 5A 57 52 49 54 45  ASC: WIZWRITE
   REMOTE TSAP-ID : LENGTH: 8     HEX: 57 5A 50 53 42 43 50 55  ASC: WZPSBCPU
   REMOTE NSAP-ID : LENGTH: 12   ASC :

   NUMBER OF JOBS PER TSAP      : 1
   