# COM PROFIBUS

## Station-oriented Address Assignment

PROFIBUS Address 4

Station Type : | DP/DP Coupler
Order Number : | 6ES7 158 0AD00 0XA0
Station Description : | S7-1500-Slave
Response Monitoring : | ON
Error-reporting Mode : | ---

Address Table for Master PS5595

Parameterization Master

Number of IM 308-C : | 16 | Area Linear
Base Address of DP Window : | FE00
Associated Host : | S5-135U / CPU 928 | 'PS5595'

Slot | ID | Remarks | Order Number | I Addr. | O Addr. | DP Window
1 | 031 |  | 16 Bytes Input | Q128 |  | 000 --
2 | 031 |  | 16 Bytes Input | Q144 |  | 016 --
3 | 031 |  | 16 Bytes Input | Q160 |  | 032 --
4 | 031 |  | 16 Bytes Input | Q176 |  | 048 --
5 | 031 |  | 16 Bytes Input | Q192 |  | 064 --
6 | 031 |  | 16 Bytes Input | Q208 |  | 080 --
7 | 031 |  | 16 Bytes Input | Q224 |  | 096 --
8 | 023 |  | 8 Bytes Input | Q240 |  | 112 --
9 | 047 |  | 16 Bytes Output |  | Q128 | -- 000
10 | 047 |  | 16 Bytes Output |  | Q144 | -- 016
11 | 047 |  | 16 Bytes Output |  | Q160 | -- 032
12 | 047 |  | 16 Bytes Output |  | Q176 | -- 048
13 | 047 |  | 16 Bytes Output |  | Q192 | -- 064
14 | 047 |  | 16 Bytes Output |  | Q208 | -- 080
15 | 047 |  | 16 Bytes Output |  | Q224 | -- 096
16 | 039 |  | 8 Bytes Output |  | Q240 | -- 112

Parameterization
User-specific Parameter Data in Hexadecimal Format

Parameter Name | Value
Diagnose | Extended diagnosis disabled