#########################################################################################
###   Overview S7 1200/1500 Function Blocks V1.10 for TIA-Portal for CLV6xx/Lector620 ###
#########################################################################################

This package contains the Function block for CLV6xx / Lector6xx using S7 1200/1500 with integrated PROFINET/PROFIBUS 
for TIA-Portal V12 SP1 or higher.

For latest or other version see "http://www.sick.com/software" and select software category “Function block”.

Using "PNDP
"  ==> Profibus and Profinet integrated in S7 CPU:
  


	(all times HS-Mode must be used)

	These devices can be connected to Profinet:
	- CLV6xx/Lector620 with Profinet on board  
	- CLV6xx/Lector620 with CDF600-22xx (2-port) (Proxy- and Gateway-Mode)
	- CLV6xx/Lector620 with CDM425

	These devices can be connected to Profibus:
	- CLV6xx/Lector620 with CDF600-21xx or CDF600-01xx (Proxy- and Gateway-Mode)
	- CLV6xx/Lector620 with CMF400-Profibus


The function block do in general:
- Receive result data	

Optional you can use these functions:
- Triggering of the device (SW-Trigger)
- Communcation test
- Set Match-Codes
- Save Parameter Set permanent
- Send Free Commands 



################################################################################################
###   Übersicht S7 1200/1500 Funktions-Bausteine V1.10 fuer TIA-Portal fuer CLV6xx/Lector620 ###
################################################################################################

Dieses Paket enthält den SICK S7 Funktionsbaustein für CLV6xx/Lector6xx für S7 1200/1500 mit integriertem PROFINET/PROFIBUS 
fuer TIA-Portal V12 SP1 oder höher.

Fuer neuste bzw. andere Versionen siehe "http://www.sick.com/software", Software category “Function block”.

Version "PNDP
"  ==> Profibus und Profinet integriert in der S7 CPU:
  


	(Es ist immer der HS-Mode zu verwenden)

	Diese Geräte können via Profinet angeschlossen werden:
	- CLV6xx/Lector620 mit Profinet on board  
	- CLV6xx/Lector620 mit CDF600-22xx (2-port) (Proxy- und Gateway-Mode)
	- CLV6xx/Lector620 with CDM425

	Diese Geräte können via Profibus angeschlossen werden:
	- CLV6xx/Lector620 mit CDF600-21xx oder CDF600-01xx (Proxy- und Gateway-Mode)
	- CLV6xx/Lector620 mit CMF400-Profibus


Der Funktionsbaustein leistet folgendes:
- Datenempfang des Leseergebnisses

Optional können folgende Funktionen verwendet werden:
- Triggererung der Gerätes (SW-Trigger)
- Kommunikationstest
- Match-Code setzen
- Parameter permanent speichern 
- Freies Kommando senden

