{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Scada Indexnummers"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Scada Indexnummers","index":0,"n_rows":149,"n_cols":2,"rows_kept":149,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Id","Alarm"]
[1,"Storing extern"]
[2,"Storing niet in"]
[3,"Storing niet uit"]
[4,"Storing flowdetectie"]
[5,"Storing niet open"]
[6,"Storing niet dicht"]
[7,"Storing draadbreuk"]
[8,"Stor. plausibiliteit"]
[9,"Storing hoog-hoog"]
[10,"Storing hoog"]
[11,"Storing laag"]
[12,"Storing laag-laag"]
[13,"Storing"]
[14,"Storing spoeltijd bewaking"]
[15,"Storing inbraakdetectie"]
[16,"Storing afwijking"]
[17,"Storing FO"]
[18,"Storing configuratie plc"]
[19,"Storing batterij plc"]
[20,"Storing I/O kaart plc"]
[21,"Storing koelunit KU-977"]
[22,"Storing capaciteit ruwpompen ondiep"]
[23,"Storing capaciteit ruwpompen diep"]
[24,"Twee ruwpompen ondiep verzamelstoring"]
[25,"Twee ruwpompen diep verzamelstoring"]
[26,"Spoelprogramma afgebroken"]
[27,"Overschrijding afvoertijd 1e filtraat"]
[28,"Verdebiet Nacht"]
[29,"Verdebiet Dag"]
[30,"reserve"]
[31,"Loss Of Echo"]
[32,"reserve"]
[33,"Water op vloer"]
[34,"Voor alarm water op vloer"]
[35,"Blokeer nivo water op vloer"]
[36,"Egalisatiekelders geblokkeerd"]
[37,"FeCL3 tanks leeg"]
[38,"twee FeCL3 doseerpompen verzamelstoring"]
[39,"Slibtanks geblokkeerd"]
[40,"Netstoring 230 VAC"]
[41,"Storing gelijkrichters 24 VDC"]
[42,"Storing elekt. by-pass (EUE)"]
[43,"MCU STORING"]
[44,"24 VDC spanning te laag"]
[45,"Storing 230 VAC"]
[46,"MBU niet auto"]
[47,"Thermistor"]
[48,"Storing MBU"]
[49,"Droogloop"]
[50,"Storing FO"]
[51,"Hoofdschakelaar FO uit"]
[52,"Wenswaarde FO niet auto"]
[53,"Klep in storing"]
[54,"Circutor         (#11)"]
[55,"Regelaar druk    (#12)"]
[56,"Regelaar flow    (#13)"]
[57,"Wago I/O RWK 11  (#21)"]
[58,"Simocode RWK 11  (#22)"]
[59,"Emotron FO RWK 11(#23)"]
[60,"Wago I/O RWK 7   (#31)"]
[61,"Simocode RWK 7   (#32)"]
[62,"Danfoss FO RWK 7 (#33)"]
[63,"Wago I/O RWK 6   (#41)"]
[64,"Simocode RWK 6   (#42)"]
[65,"Emotron FO RWK 6 (#43)"]
[66,"Glasbox Energiegebouw"]
[67,"Glasbox rwk 6"]
[68,"Glasbox rwk 7"]
[69,"Glasbox rwk 11"]
[70,"Hoofdschakelaar uit  "]
[71,"Storing 230 VAC BK01"]
[72,"Trafo 1"]
[73,"Trafo 2"]
[74,"Trafo 3"]
[75,"Trafo 4"]
[76,"Nedalo installatie"]
[77,"ventilator 1"]
[78,"ventilator 2"]
[79,"droogloop beveiliging"]
[80,"bedieningslucht pompgebouw"]
[81,"bedieningslucht"]
[82,"noodbedrijf P-501"]
[83,"noodbedrijf P-502"]
[84,"noodbedrijf P-503"]
[85,"noodbedrijf P-504"]
[86,"noodbedrijf P-507"]
[87,"noodbedrijf P-508"]
[88,"MBU P-501"]
[89,"MBU FP-502"]
[90,"MBU FP-503"]
[91,"MBU P-504"]
[92,"MBU P-507"]
[93,"MBU P-508"]
[94,"REGELAAR TORENDRUK"]
[95,"REGELAAR LEIDINGKARATERISTIEK"]
[96,"FO FP-502"]
[97,"FO FP-503 "]
[98,"W.o.v. watertoren "]
[99,"Temp. best. kast hoog"]
[100,"Wisselricht. storing"]
[101,"Dieplaadrel. afgev."]
[102,"Hand by-pass aan"]
[103,"Ventilator storing   "]
[104,"Blok.stappen          "]
[105,"Glaszekering"]
[106,"HS AR01 201/2"]
[107,"KwH meter PKZM AR01 201/4"]
[108,"PKZM'S AR01 400V"]
[109,"PKZM'S AR01 230V"]
[110,"reserve"]
[111,"HS trafo 1-4"]
[112,"HS trafo 1/2"]
[113,"HS trafo 3/4"]
[114,"reserve"]
[115,"Nedalo 1"]
[116,"Nedalo 2"]
[117,"Persoonbeveiliging"]
[118,"Negatieve puls"]
[119,"Geschakelde null"]
[120,"24V voeding 1"]
[121,"24V voeding 3"]
[122,"reserve"]
[123,"24V voeding 2"]
[124,"24V voeding 4"]
[125,"Storing hoog/laag"]
[126,"Storing nobreak 1"]
[127,"Storing nobreak 2"]
[128,"Slangbreuk/maxdruk "]
[129,"Storing Werkschakelaar"]
[130,"Storing Stuurstroom"]
[131,"Storing Thermisch"]
[132,"Rack 1"]
[133,"Rack 2"]
[134,"Rack 3"]
[135,"Rack 4"]
[136,"Communicatie"]
[137,"Handbediening actief"]
[138,"Temperatuur alarm"]
[139,"Noodstop"]
[140,"Koppeling niet oke"]
[141,"Storing tracing"]
[142,"Storing ruimteverwarming"]
[143,"Storing Overspanning beveiliging"]
[144,"Storing Verlichting"]
[145,"Storing Noodverlichting"]
[146,"Test Primair Alarm"]
[147,"Test Secundair Alarm"]
[148,"Niet auto"]