{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PLC 02 - Productie"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PLC 02 - Productie","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Tag","I/O-adres","PLC Tag","Scada Tag","Communicatie","Ondergrens","Bovengrens","Eenheid","Omschrijving"]
["PIT-605-01",300001,"PIT-605-01_Inh","PLC02_PIT60501_Meetw","Analoog in","0","10000","m3","Inhoud RWK 05 Inhoud"]
["PIT-606-01",300004,"PIT-606-01_Inh","PLC02_PIT60601_Meetw","Analoog in","0","10000","m3","Inhoud RWK 06 Inhoud"]
["PIT-607-01",300005,"PIT-607-01_Inh","PLC02_PIT60701_Meetw","Analoog in","0","10000","m3","Inhoud RWK 07 Inhoud"]
["PIT-608-01",300009,"PIT-608-01_Inh","PLC02_PIT60801_Meetw","Analoog in","0","10000","m3","Inhoud RWK 08 Inhoud"]
["PIT-611-01",300010,"PIT-611-01_Inh","PLC02_PIT61101_Meetw","Analoog in","0","10000","m3","Inhoud RWK 11 Inhoud"]
["FITR-330-01",300011,"FITR-330-01_Deb","PLC02_FITR33001_Meetw","Analoog in","0","1500","m3/h","Debiet spoellucht Debiet"]
["PITR-330-01",300012,"PITR-330-01_Druk","PLC02_PITR33001_Meetw","Analoog in","0","1000","bar","Druk spoellucht Druk"]
["FIT-301-0",300013,"FIT-301-01_Deb","PLC02_FIT30101_Meetw","Analoog in","0","1000","m3/h","Debiet Spoelwaterpomp 1 Debiet"]
["FIT-302-01",300014,"FIT-302-01_Deb","PLC02_FIT30201_Meetw","Analoog in","0","1000","m3/h","Debiet Spoelwaterpomp 2 Debiet"]
["",300015,"",null,"Analoog in","","","",""]
["PTI-670-01",300016,"PTI-670-01_Druk","PLC02_PTI67001_Meetw","Analoog in","0,0","10,0","bar","Drukmeting Bedrijfslucht Druk"]
["",300017,"",null,"Analoog in","","","",""]
["",300018,"",null,"Analoog in","","","",""]
["",300019,"",null,"Analoog in","","","",""]
["",300020,"",null,"Analoog in","","","",""]
["",300021,"",null,"Analoog in","","","",""]
["QIT-212-02",300022,"QIT-212-02_Trbl","PLC02_QIT21202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 1 Troebelheid"]
["QIT-222-02",300023,"QIT-222-02_Trbl","PLC02_QIT22202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 2 Troebelheid"]
["QIT-232-02",300024,"QIT-232-02_Trbl","PLC02_QIT23202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 3 Troebelheid"]
["QIT-242-02",300025,"QIT-242-02_Trbl","PLC02_QIT24202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 4 Troebelheid"]
["QIT-252-02",300026,"QIT-252-02_Trbl","PLC02_QIT25202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 5 Troebelheid"]
["QIT-262-02",300027,"QIT-262-02_Trbl","PLC02_QIT26202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 6 Troebelheid"]
["QIT-272-02",300028,"QIT-272-02_Trbl","PLC02_QIT27202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 7 Troebelheid"]
["QIT-282-02",300029,"QIT-282-02_Trbl","PLC02_QIT28202_Meetw","Analoog in","0,00","2,50","NTU","Troebelheidsmeting Nafilter 8 Troebelheid"]
["",300030,"",null,"Analoog in","","","",""]
["",300031,"",null,"Analoog in","","","",""]
["",300032,"",null,"Analoog in","","","",""]
["",null,"",null,null,"","","",""]
["",null,"",null,null,"","","",""]
["",null,"",null,null,"","","",""]
["",null,"",null,null,"","","",""]
["",null,"",null,null,"","","",""]