{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PLC 02 - Productie"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PLC 02 - Productie","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Tag","I/O-adres","PLC Tag","Scada Tag","Communicatie","Ondergrens","Bovengrens","Eenheid","Omschrijving"]
["FC-111-01","400001","FC-111-01_SP_Flow","PLC02_FC11101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 1 Setpoint Flow"]
["FC-121-01","400002","FC-121-01_SP_Flow","PLC02_FC12101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 2 Setpoint Flow"]
["FC-131-01","400003","FC-131-01_SP_Flow","PLC02_FC13101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 3 Setpoint Flow"]
["FC-141-01","400004","FC-141-01_SP_Flow","PLC02_FC14101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 4 Setpoint Flow"]
["FC-151-01","400005","FC-151-01_SP_Flow","PLC02_FC15101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 5 Setpoint Flow"]
["FC-161-01","400006","FC-161-01_SP_Flow","PLC02_FC16101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 6 Setpoint Flow"]
["FC-171-01","400007","FC-171-01_SP_Flow","PLC02_FC17101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 7 Setpoint Flow"]
["FC-181-01","400008","FC-181-01_SP_Flow","PLC02_FC18101","Analoog uit","0,0","600,0","m3/h","Debietregelaar Ruwwater Voorfilter 8 Setpoint Flow"]
["_2 PROD","400009","_2 PROD_Tot_Deb","PLC02_2 PROD","Analoog uit","0","4800","m3/h","Productie Totaal Debiet"]
["SPW","400010","SPW_Tot_Deb","PLC02_SPW","Analoog uit","0","2000","m3/h","Spoelwater Totaal Debiet"]
["FC-301-02","400011","FC-301-02_SP_Flow","PLC02_FC30102","Analoog uit","0","600","m3/h","Debietregelaar Spoelwaterpomp 1 Setpoint Flow"]
["FC-302-02","400012","FC-302-02_SP_Flow","PLC02_FC30202","Analoog uit","0","600","m3/h","Debietregelaar Spoelwaterpomp 2 Setpoint Flow"]
["V-331","400013","V-331_Setp","PLC02_V331","Analoog uit","0","1000","m3/h","Spoelluchtblower 1 Setpoint"]
["V-332","400014","V-332_Setp","PLC02_V332","Analoog uit","0","1000","m3/h","Spoelluchtblower 2 Setpoint"]
["","400017","","","Analoog uit","","","",""]
["","400018","","","Analoog uit","","","",""]
["SPW","400019","SPW_Tot_F1",null,"Analoog uit","0","1000","m3/h","Spoelwater Totaal Debiet (F1)"]
["SPW","400020","SPW_Tot_F3",null,"Analoog uit","0","1000","m3/h","Spoelwater Totaal Debiet (F3)"]
["SPW","400021","SPW_Tot_F5",null,"Analoog uit","0","1000","m3/h","Spoelwater Totaal Debiet (F5)"]
["SPW","400022","SPW_Tot_F7",null,"Analoog uit","0","1000","m3/h","Spoelwater Totaal Debiet (F7)"]
["SPW","400023","SPW_Tot_F8",null,"Analoog uit","0","1000","m3/h","Spoelwater Totaal debiet (F8)"]
["SPL","400024","SPL_Tot_F1",null,"Analoog uit","0","1000","m3/h","Spoellucht Totaal Debiet (F1)"]
["SPL","400025","SPL_Tot_F3",null,"Analoog uit","0","1000","m3/h","Spoellucht Totaal Debiet (F3)"]
["SPL","400026","SPL_Tot_F5",null,"Analoog uit","0","1000","m3/h","Spoellucht Totaal Debiet (F5)"]
["SPL","400027","SPL_Tot_F7",null,"Analoog uit","0","1000","m3/h","Spoellucht Totaal Debiet (F7)"]
["KALK","400028","KALK_Inh_T1",null,"Analoog uit","0","400","m3","Kalkmelk installatie Inhoud tank 1"]
["KALK","400029","KALK_Inh_T2",null,"Analoog uit","0","400","m3","Kalkmelk installatie Inhoud tank 2"]
["RWB","400030","RWB_Tot_Inh",null,"Analoog uit","0","27000","m3","Reinwaterberging Totaal inhoud"]
["RWT","400031","RWT_Tot_Afg",null,"Analoog uit","0","10000","m3/h","Reinwatertransport Totaal afgifte"]
["","400032","",null,"Analoog uit","","","",""]
["",null,"",null,null,"","","",""]
["",null,"",null,null,"","","",""]